{"text_format":"1","workbook":"xls","n_sheets":1,"sheets":["O1-O2 répartition de charge uniforme"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":1,"defined_names":1,"comments":4,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"O1-O2 répartition de charge uniforme","index":0,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[[0,1,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[5,2,5,5],[6,2,6,5],[7,2,7,5],[9,1,9,6],[10,2,10,3],[11,2,11,3],[14,1,14,6],[17,3,19,3],[22,1,22,6],[27,1,27,6],[28,1,28,2],[29,1,29,3],[30,1,30,4],[31,1,31,4],[31,5,32,5],[32,1,32,3],[34,1,34,6],[38,1,38,6],[45,2,45,5],[46,2,46,5],[47,2,47,5]],"flags":["formulas_cached_only"]}
[null,"REMORQUE O1/O2 A ESSIEUX CENTRAUX\nCALCUL DE RÉPARTITION DE CHARGES UNIFORME"]
[null,"CENTRE AXLE O1/O2 TRAILER – UNIFORM LOAD DISTRIBUTION"]
[]
[null,"REMPLIR LES CASES GRISES / Fill the grey cells"]
[null,"CARACTÉRISTIQUES DU VÉHICULE"]
[null,"Marque / Make"]
[null,"Type"]
[null,"N° d’identification / VIN"]
[]
[null,"MASSES"]
[null,null,"Poids total autorisé en charge / maximum laden mass",null,"PTAC ="]
[null,null,"Poids à vide / empty mass",null,"PV =",0]
[null,null,"Chargement / loading capacity",null,"Ch = PTAC – PV =",0]
[]
[null,"CALCUL DE L’EMPATTEMENT THÉORIQUE / theoretical wheelbase calculation"]
[null,null,"Capacité","Théorie"]
[null,"0-Tête d’attelage / coupling head",null,0,null,"Distance"]
[null,"1-Essieu / axle",null,0,"0-1 : Tête d'attelage à essieu 1"]
[null,"2-Essieu / axle",null,null,"1-2 : Essieu 1 à essieu 2"]
[null,"3-Essieu / axle",null,null,"2-3 : Essieu 2 à essieu 3"]
[null,null,null,null,"Empattement théorique F'=",0]
[]
[null,"DIMENSIONS DU VÉHICULE CARROSSÉ (HORS TOUT)"]
[null,null,null,"Longueur / Length","L ="]
[null,null,null,"Largeur / Width"," l ="]
[null,null,null,"Surface","L*l =",0]
[]
[null,"CARACTÉRISTIQUES DE LA CARROSSERIE / bodywork caracteristics"]
[null,"Longueur utile de chargement / useful length of cargo area",null,null,"T ="]
[null,"Porte-à-faux arrière utile / length of the useful rear overhang of the cargo area",null,null,"W ="]
[null,"Porte-à-faux arrière utile théorique / theoretical length of the useful rear overhang of the cargo area                             Xu =",null,null,null,{"$error":"#VALUE!"}]
[null,"Distance du centre de gravité du chargement à l’axe de la force, appliquée au sol par l’essieu arrière théorique : ",null,null,null,{"$error":"#VALUE!"}]
[null,"Distance from the centre of gravity of the cargo to the theoretical rear axle",null,null," Y = T/2 – Xu ="]
[]
[null,"RÉPARTITION DU POIDS DU CHARGEMENT / load distribution"]
[null,null,"Sur la tête d’attelage / on the coupling head",null,"Ch AV = Ch * Y/F’ =",{"$error":"#VALUE!"}]
[null,null,"Sur le(s) essieu(x) arrières / on the rear axle(s)",null,"Ch AR = Ch *(F’-Y)/F’ =",{"$error":"#VALUE!"}]
[]
[null,"RÉPARTITION DU POIDS TOTAL EN CHARGE (PTAC) / maximum laden mass distribution"]
[]
[null,"Poids à vide avant","front empty mass",null,"Poids à vide arrière","rear empty mass"]
[null,"Chargement avant","front loading",{"$error":"#VALUE!"},"Chargement arrière","rear loading",{"$error":"#VALUE!"}]
[null,"Poids total avant","total front mass",{"$error":"#VALUE!"},"Poids total arrière","rear total mass",{"$error":"#VALUE!"}]
[null,"Poids avant maximal","front maximal mass",0,"Poids arrière maximal","rear maximal mass",0]
[]
[null,"Fait à :"]
[null,"Le :"]
[null,"Signature et cachet :"]